

**EKO H**

**Product Description**

*EKO H is very effective purging agent. Non-Corrosive, Non-Abrasive and Non-Toxic designed to clean materials with high working temperatures 230°C –360°C: PP, PE, PA, PC, PS, EVOH, ULTEM, PEX, PPO, PPS, Polysulfane and more.*

**Product information**

|  |  |  |  |
| --- | --- | --- | --- |
| PHYSICAL | Unit | Test Method | Property Value |
| Filler content | % | ISO 3451-1 | 20 |
| Bulk Density | Kg/Lit | INTERNAL | 1.4 |
| Moisture Content | ppm | INTERNAL | <1500 |

Date: 26.09.17

Version: A

The information contained in this document supplied in good faith. However it is given purely as an indication. It shall not be construed in any way as formal commitment or warranty on our part. Notably in respect of the eventual infringement of any rights of third parties who may use our products.

We remain at your entire disposal to provide you with any information that you might require.